**深圳市帕骐电子科技有限公司**

**产品部-10新品上架描述表**

**1.Key Features**

（Red marked content must be show on Listing Title or Bullet Point ）

**产品描述**（字体颜色为红色代表要填写在标题或者短描述Bullet Point ）

**1）**Android **5.1 Lollipop** , CPU: Rockchip PX3 Cortex A9 Quad Core 1.6GHz, Optimized Radio IC:NXP TEF6686,

安卓5.1操作系统，四核CPU，高品质的收音IC:NXP TEF6686

**2）**Support 1080P HD video, support **DAB+** Digital Radio(Extra DAB+ box required)，support mirror link function, You can use your smartphone's online GPS to mirror on this unit

支持播放1080P 视频 ，支持数字收音机，支持mirror link, 可以把手机的在线导航显示在机器上，

**3）**Support GPS Navigation(map software or app not included), Built in USB Port/ Micro SD Slot, WIFI(Built in WIFI modem)/3G(Extra device required), Support reversing camera(Extra device required)

支持GPS功能，内置USB/SD卡槽，内置wifi模块，支持3G网络（要求额外的设备），支持倒车摄像头功能（摄像头选配）

**4）**Please compare the dimensions, shape of this unit with the central console before purchasing, in case it does not fit the size.

购买前请先核对机子的形状和尺寸

**5）**Support Bluetooth call /audio play, Sync phonebook，external microphone, Support output almost everything to the headrests, even it play the video from USB/SD card, or online youtube video.

支持蓝牙通话，蓝牙音乐，支持同步电话本和支持外置麦克风,支持几乎所有界面输出到头枕。

1. **Technical Specification技术参数**

Item Description:

6.95" Android 5.1 Lollipop Quad Core 1.6GHz Car Stereo DVD Player for Toyota Series

Applicable Models：The following car model and year are for reference ,please make sure your original car radio has the same shape as our unit.

TOYOTA RAV4 2001-2005

TOYOTA HILUX 2005-2010

TOYOTA Terios 2006-2012

TOYOTA FJ CRUISER 2007-2010

TOYOTA YARIS 2005-2011

TOYOTA Rush 2006-2012

TOYOTA ALPHARD

TOYOTA VIOS

TOYOTA Echo 1998-2005

TOYOTA PREVIA GL

TOYOTA Tundra 2000-2006

TOYOTA VIZI 1998-2005

TOYOTA HIACE

TOYOTA HIGHLANDER 2001-2007

TOYOTA Vitz 1998-2005

TOYOTA IELAS

TOYOTA CELICA

TOYOTA Soluna Vios 2003-2007

TOYOTA FORTUNER 2006-2012

TOYOTA MR2 2002-2012

TOYOTA INNOVA

TOYOTA 4RUNNER 2003-2009

Dailhatsu Be-go 2006-2012

TOYOTA COROLLA 2002-2006

TOYOTA SEQUOIA 2001-2007

Dailhatsu Terios Eco 2006-2012

TOYOTA CAMRY 1999-2005

TOYOTA KLUGER 2002-2007

Daihatsu Terios Wild 2006-2012

TOYOTA LAND CRUISER

Perodua Nautica 2006-2012

Alert:

If your car has original JBL system, you would need the JBL decoder from us.

Specifications：

General:

OS: Android 5.1 Lollipop

CPU: Rockchip PX3 Cortex A9 Quad Core 1.6GHz

RAM: DDR3 1GB

Nand Memory: 16GB

Radio IC:NXP TEF6686

Bluetooth IC: BC6

Audio output: 4\*50W max

Screen Resolution: 800\*480

Cold Boot time: about 25-30s

Screen:

Screen Size: 6.95-Inch Digital Screen

Resolution: 800\*480

Capacitive Touch Screen (5 points)

Image Brightness /Contrast/ Color Adjustable

Phone Mirroring

Mirror your phone on the 6.95 inch screen .

For Android phone ,you can mirror and control on the unit via USB cable connection ,  
Air Play For iPhone, you can just mirror on the unit via wifi  connection ,can not control

GPS：

Support online and off-line navi app, support 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/SD playback while navigating.)

DVD:

DVD drive: Region Free

Compatible Formats:

AVI/DVD/DVD+R/DVD-R/DVD+RW/DVD-RW/VCD/MP3/CD/CD-RW/JPEG etc.

AV Output

For this unit ,it can display almost everything to your headrests, even you play the video from USB/SD card . or online youtube video, Many headunits in the market can only display the DVD video to the headrest.

Bluetooth:

Built-In Microphone in the control panel for hands free calling function

External microphone also included for free clear voice calling

Support Bluetooth audio player/Phone Book function

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Support Bluetooth Connection for iPhones/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

Radio

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in USB Port/Micro SD Slot

USB Port: support USB drive up to 32GB

Micro SD Card Slot: support micro SD Card up to 32GB

Support Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Support Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

EQ

Max audio output: 4 X 50W ,

Signal-To-Noise Ratio:>85db

OSD Language:

English, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, German, French, Thai, Hebrew, Danish，Hungarian，Dutch，Polish，Finnish，Greek，Bulgarian，Belgian，Swedish，etc.

DAB+ Digital Radio (Extra DAB+ box required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle. Permanent increase in channels and expansion of the station area soon make DAB accessible to most of Europe.

(If interested ,please buy the DAB+ box from us)

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034 on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI/3G(Extra device required)

3G: Require external USB 3G modem (Search Y0014 on our store) and your local Internet SIM card to be connected

Support WCDMA/CDMA2000/TD-SCDMA 3G bandwidth

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

DVR (Extra device required)

Built in USB port for USB Camera (Search Y0020 on our store) input for video record

Storage Router: Save in micro SD card from the Map SD slot

(Attention: only for video record, it cannot record audio)

Cam-In(Extra device required)

Support RCA type reverse camera input

1. **Instruction 使用说明**

面板的顶部最大长度是204mm（最小200mm）, 面板最大高度是104mm（最小100mm）金属机身部分的长度是153mm, 高度是100mm，宽度是178mm，

1. **Package包装**

**5.Reference Link参考链接**