**深圳市帕骐电子科技有限公司**

**产品部-10新品上架描述表**

**1.Key Features**

（Red marked content must be show on Listing Title or Bullet Point ）

**产品描述**（字体颜色为红色代表要填写在标题或者短描述Bullet Point ）

**1）**Android **6.0 Marshmallow** , CPU: Cortex A7 Quad Core 1.6GHz , High quality radio IC: NXP TEF6686 ,with good radio reception. motorized screen， adjustable angle screen,you can change it as you prefer.

安卓6.0操作系统，四核CPU，高品质的6686收音IC，效果更好，屏幕角度可调

**2）Supports subwoofer audio output, and control it separately.**

Supports 1080P HD video,supports phone mirroring function,You can use your smartphone's online GPS to mirror on this unit,support **DAB+** function

支持重低音输出，并可以单独调节，支持播放1080P 视频，支持手机互联, 可以把手机的在线导航显示在机器上，支持DAB数字收音机，

**3）**Supports GPS Navigation(map software or app not included), Built in USB Port/ Micro SD Slot(**up to 64GB**), WIFI(Built in WIFI modem)/3G(Extra device required), Support reversing camera(Extra device required)

支持GPS功能，内置USB/SD卡槽（最大支持64GB），内置wifi模块，支持3G网络（要求额外的设备），支持倒车摄像头功能（摄像头选配）

**4）P**lease compare the dimensions, shape of our unit with the central console before purchasing, in case it does not fit for your car.

购买前还请先核对机子的形状和尺寸

**5)** Supports Bluetooth call /audio play,Sync phonebook,quick search contacts, Comes with 1.5m long WIFI antenna for better signal reception.

 支持蓝牙通话，蓝牙音乐，支持同步电话本,快速搜索联系人，配有1.5米长的wifi天线，让机子更好的接收wifi信号

**6)** 支持ipod/iphone音频输入, 支持DVR

Support iphone/ipod audio input by USB. Support DVR function.

1. **Technical Specification技术参数**

Item Description:

7" Multi-touch motorized Screen Quad Core 1.6GHz Android 6.0 Marshmallow Car DVD Player

Attention: please make sure your original car radio has the same shape as our unit.

Specifications：

General:

OS: Android 6.0 Marshmallow

CPU: Cortex A7 Quad Core 1.6GHz

RAM: DDR3 1GB

Nand Memory: 16GB

Radio IC: NXP TEF6686

Bluetooth: BT 4.0

Working Voltage: 10.8~14.8V DC

Audio output: 4\*45W Max

Cold Boot time: about 25s

Blue-color button light

Screen:

Screen Size: 7 Inch Digital Screen

Screen Resolution: 1024\*600

Capacitive Touch Screen (5 points)

Image Brightness /Contrast

Operation System

This unit is powered by Android 6.0 system, and API/SDK is 23, Cortex A7 Quad Core CPU, 1.6GHz, which will provide you a different experience than before.

DAB+ Digital Radio (Extra DAB+ box Y0251 required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle.

which make DAB broadly accessible to most of Europe.

EQ

**Supports subwoofer audio output, and control it separately.**

Max audio output: 4 X 45W ,

Support iphone/ipod audio input by USB cable.

Support models: iPod Nano7/iPodTouch4/iPod shuffle 5,6,7/iPhone 5, 5S,6, 6S,7.

Phone Mirroring

Mirror your phone on the 7 inch screen .

For Android phone ,you can mirror and control on the unit via USB cable connection ,
Air Play For iPhone, you can just mirror on the unit via wifi connection ,can not control

(Support Android 7.1 smart phone, support iOS 10.3 iPhone.)

GPS：

Supports online and off-line navi app, supports 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/SD playback while navigating.)

Bluetooth 4.0 :

Built-In Microphone in the control panel for hands free calling function

Supports Bluetooth audio player/sync Phone Book/quick search contacts function

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Supports Bluetooth Connection for iPhones/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

(Attention: Only support resistance based analog signal input steering wheel)

Radio

High quality radio IC: NXP TEF6686 ,with good radio reception.

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in SD card slot/ USB Port

Supports SD card/ USB drive up to 64GB with FAT32 or ntfs format

Supports Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Supports Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

OSD Language:

English, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, German, French, Thai, Hebrew, Danish，Hungarian，Dutch，Polish，Finnish，Greek，Bulgarian，Belgian，Swedish，etc.

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034 on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI/3G internet

3G: Require external USB 3G modem (Search Y0014 on our store) and your local Internet SIM card to be connected，Only support WCDMA 3G bandwidth

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

（It comes with 1.5m long WIFI antenna for better signal reception.）

Cam-In(Extra device required)

Supports reverse camera input , automatically trigger to reverse camera when reversing the car. (Only support RCA type reverse camera input ).

1. **Instruction 使用说明**
2. **Package包装**

**5.Reference Link参考链接**