**深圳市帕骐电子科技有限公司**

**产品部-10新品上架描述表--AA0479B**

1. **Key Features**

(Red marked content must be show on Listing Title or Bullet Point.)

**产品描述**（字体颜色为红色代表要填写在标题或者短描述。）

1. Android**10**, RAM:4GB ROM:64GB, CPU: Octa-core Processor, High quality radio IC: NXP6686 ,with better reception.

安卓10操作系统，4+64G内存，八核CPU，高品质的6686收音IC，效果更好。

1. .G+G double layer glass touch screen with Anti-Glare function for enjoyable touch experience。

G+G双层玻璃触摸屏，带防眩光功能，使用户触摸体验更好。

**3)** Built-in Qualcomm Bluetooth 5.0 clip **,**Support Bluetooth call /audio play, Sync phonebook, external microphone. only support DVD video to your headrests

内置高通蓝牙5.0芯片，支持蓝牙通话，蓝牙音乐，支持同步电话本和支持外置麦克风。只支持DVD视频输出

**4)** Support 1080P HD video, Supports subwoofer audio output, and control it separately, support mirror link function, You can use your smartphone's online GPS to mirror on this unit, support DAB+ function.

支持播放1080P视频，支持重低音输出，并可以单独调节，支持mirror link，可以把手机的在线导航显示在机器上，支持DAB数字收音广播。

**5)** Support GPS Navigation (map software or app not included), Built in USB Port/ Micro SD Slot (**up to 64GB**), WIFI (Built in WIFI modem), Support reversing camera (Extra device required).

支持GPS功能，内置USB/SD卡槽（最大支持64GB），内置Wi-Fi模块，支持倒车摄像头功能（摄像头选配）。

**6) Support Fast-boot.** After the installation, this machine only need about 1 seconds to finish booting from the 2nd time. (Other machines typically take 30 seconds.)

支持快速开机，在安装好机器后，第二次开始，机器的启动时间会在1秒左右启动完成。（而其他的机器则通常需要30秒才能启动完成。）

**7)** Please compare the dimensions, shape of this unit with the central console before purchasing, in case it does not fit the size.

购买前请先核对机子的形状和尺寸。

**2.Technical Specification技术参数**

Item Description:

6.2" Double Din Touchscreen Octa-Core Android 10 Oreo Car Stereo DVD Player & RAM:4GB/ROM:64GB

Attention: please make sure your original car radio has the same shape as our unit.

Specifications:

General:

OS: Android 10

CPU:Octa-core Processor

RAM: DDR3 4GB

Nand Memory: 64GB

Radio IC: NXP TEF6686

Bluetooth: BT 5.0

Audio output: 4\*50W max

Cold Boot time: about 25-30s

Boot time(2nd time): about 1s

EQ

**Supports subwoofer audio output, and control it separately.**

Max audio output: 4 X 50W,

Signal-To-Noise Ratio: >55db

Multi-color button light

Panel buttons light RGB color are available, Already preset 7 colors of indicator buttons, you may change it freely, you can also set other colors to match your car.

Screen:

Screen Size: 6.2-Inch Screen

Resolution: 800\*480

Capacitive Touch Screen (5 points)

Image Brightness /Contrast/ Color Adjustable

Phone Mirroring

Mirror your phone on the 6.2 inch screen.

For Android phone, you can mirror and control on the unit via USB cable connection ,
Air Play For iPhone, you can just mirror on the unit via Wi-Fi connection, cannot control

GPS:

Support online and off-line navigation app, support 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/ playback while navigating.)

DAB+ Digital Radio (Extra DAB+ box NA7001B required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle.

which make DAB broadly accessible to most of Europe.

AV Output

For this unit,only support DVD video to your headrests.

Qualcomm Bluetooth 5.0 :

Built-In Microphone in the control panel for hands free calling function

External microphone also included for free clear voice calling

Support Bluetooth audio player/Phone Book function

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Support Bluetooth Connection for iPhones/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

(Attention: Only support resistance based analog signal input steering wheel)

Radio

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in micro SD card slot/ USB Port

Support SD card/ USB drive up to 64GB with FAT32 or ntfs format

Support Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Support Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

OSD Language:

English, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, German, French, Thai,Hebrew,Danish,Hungarian,Dutch,Polish,Finnish,Greek,Bulgarian,Belgian,Swedish,

etc.

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034/VE001B on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

(It comes with 1.5m long WIFI antenna for better signal reception.)

Cam-In(Extra device required)

Support RCA type reverse camera input

1. **Instruction 使用说明**
2. **Package包装**

**5.Reference Link参考链接**