**深圳市帕骐电子科技有限公司**

**产品部新品上架描述表——AA0461B**

**1.Key Features**

（Red marked content must be show on Listing Title or Bullet Point ）

**产品描述**（字体颜色为红色代表要填写在标题或者短描述Bullet Point ）

1）Android **9.0 Pie**, RAM:4GB, ROM:32GB, CPU: 8-Core 64-bit CPU Coretex-A53 @1.5G, High quality radio IC: NXP TEF6686 ,with good radio reception.

安卓9.0操作系统，4G+32G内存，8核CPU，高品质的6686收音IC，接收效果更好。

2）Built-in TDA7851L amplifier IC，Supports subwoofer audio output, and control it separately. Screen Resolution: 1024\*600，Support 4K/1080P HD video, support mirror link function, You can use your smartphone's online GPS to mirror on this unit, support DAB+ function(optional)

支持重低音输出，并可以单独调节,1024\*600高清屏，支持播放4K/1080P 视频 ，支持mirror link, 可以把手机的在线导航显示在机器上，支持DAB数字收音广播(选配)

3）Support output DVD or AUX video to the headrests, even it play the video from USB/SD card, or online Youtube video. Built in USB Port/ Micro SD Slot(up to 128GB), WIFI(Built in WIFI modem)/4G(Extra device required), Support reversing camera(Extra device required)

支持播放DVD或AUX视频输出到头枕, 内置USB/SD卡槽（最大支持128GB），内置wifi模块，支持4G网络（要求额外的设备），支持倒车摄像头功能（摄像头选配）

4）Checking the measurement before purchasing to ensure it fits the dashboard.

购买前还请先核对机子的形状和尺寸

5) Support Bluetooth call /audio play, Sync phonebook，quick search contacts, external microphone, Support GPS Navigation(map software or app not included),

支持蓝牙通话，蓝牙音乐，支持同步电话本,快速搜索联系人和支持外置麦克风,支持GPS。

6) Support Fast-boot. After the installation, this machine only need about 1 seconds to finish booting from the 2nd time.(Other machines typically take 30 seconds）

支持快速开机。在安装好机器后，第二次开始，机器的启动时间会在1秒左右启动完成（而其他的机器则通常需要30秒才能启动完成）

1. **Technical Specification技术参数**

Item Description:

7" Touchscreen Octa-Core Android 9.0 Car Stereo with RAM:4GB/ROM:32GB for Benz B200 Series

Applicable Models：

The following car model and year are for reference, please make sure your original car radio has the same shape as our unit.

Benz A class W169 2004-2012

Benz W639 2006-2012

Benz B class W245 2005-2012

Mercedes-Benz Viano 2006-2012

Mercedes-Benz Vito 2006-2012

Benz W906 2006-2012

Specifications：

OS: Android 9.0 Pie

CPU: 8-Core 64-bit CPU Coretex-A53 @1.5G

RAM: 4GB

ROM: 32GB

Radio IC: NXP6686

Bluetooth: BT 4.0

Working Voltage: 10.8~14.8V DC

Audio output: 4\*50W Max

Boot time (2nd time): about 1s

Screen:

Screen Size: 7-Inch Digital Screen

Resolution: 1024\*600

Capacitive Touch Screen (5 points)

Image Brightness /Contrast/ Color Adjustable

Operation System

This unit is powered by Android9.0 system, 8-Core 64-bit CPU Coretex-A53 @1.5G,

which will provide you a different experience than before.

EQ

Built-in TDA7851L amplifier IC，Supports subwoofer audio output, and control it separately.

Max audio output: 4 X 50W,

Phone Mirroring

Mirror your phone on the 7 inch screen.

For Android phone ,you can mirror and control on the unit via USB cable connection ,  
Air Play For iPhone, you can just mirror on the unit via wifi  connection ,can not control

GPS：

Support online and off-line navi app, support 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/SD playback while navigating.)

DAB+ Digital Radio (Extra DAB+ box NA7001B required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle.

which make DAB broadly accessible to most of Europe.

AV Output

For this unit, it can output the DVD or AUX video to the headrest.

Bluetooth 4.0:

Built-In Microphone in the control panel for hands free calling function

External microphone also included for free clear voice calling

Support Bluetooth audio player/Phone Book function, quick search contacts.

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Support Bluetooth Connection for iPhone/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

Radio

High quality radio IC: NXP6686, with good radio reception.

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in micro SD card slot/ USB Port.

Support SD card/ USB drive up to 128GB.

Support Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Support Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

OSD Language:

English, German, French, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, Thai, Hebrew, Danish，Hungarian，Dutch，Polish，Finnish，Greek，Bulgarian，Belgian，Swedish，Japanese，etc.

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034 on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI/4G internet

4G internet (Extra device required)

Support 4G internet, Require external USB 4G modem.

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

（It comes with 1.5m long WIFI antenna for better signal reception.）

Cam-In(Extra device required)

Support RCA type reverse camera input, automatically trigger to reverse camera when reversing the car.

DVD

Support all formats

DVD drive: Region Free

Compatible Formats: AVI/DVD/DVD+R/DVD-R/DVD+RW/DVD-RW/VCD/MP3/CD/CD-RW/JPEG etc.

**3.Instruction 使用说明**

**4.Package包装**

**5.Reference Link参考链接**