**深圳市帕骐电子科技有限公司**

**产品部-新品上架描述表-AA0406B**

1. **Key Features**

**产品描述**:

1. Android 9.0 Pie,RAM:4GB, ROM: 64GB. CPU: Octa-Core Processor, High quality radio IC: NXP6686, with good radio reception.

安卓9.0操作系统，4G+64G内存，8核CPU，高品质的6686收音IC，效果更好。

2）Built-in TDA7851L amplifier IC, Supports subwoofer audio output. Screen Resolution: 1024\*600, Support 4K/1080P HD video, support mirror link function. You can use your smartphone's online GPS to mirror on this unit, support DAB+ function(optional).

支持重低音输出，并可以单独调节，1024\*600高清，支持播放4K/ 1080P 视频，支持mirror link，可以把手机的在线导航显示在机器上，支持DAB数字收音广播(选配)。

3）Support output almost everything to the headrests, even it play the video from USB/SD card, or online YouTube video. Built in USB Port/ Micro SD Slot (up to 128GB), WIFI (Built in WIFI modem)/4G (Extra device required), Support reversing camera(Extra device required).

支持几乎所有界面输出到头枕，内置USB/SD卡槽（最大支持64GB），内置wifi模块，支持3G网络（要求额外的设备），支持倒车摄像头功能（摄像头选配）。

4）Please compare the dimensions, shape of our unit before purchasing, in case it does not fit the dashboard.

购买前还请先核对机子的形状和尺寸。

5) Support Bluetooth call/audio play, Sync phonebook, quick search contacts, and external microphone. Support GPS Navigation (map software or app not included).

支持蓝牙通话，蓝牙音乐，支持同步电话本，快速搜索联系人和支持外置麦克风，支持GPS。

6) Support Fast-boot. After the installation, this machine only need about 1 second to finish booting from the 2nd time. (Other devices typically take 30 seconds.）

支持快速开机。在安装好机器后，第二次开始，机器的启动时间会在1秒左右启动完成（而其他的机器则通常需要30秒才能启动完成）。

1. **Technical Specification技术参数**

Item Description:

7" Touchscreen Octa Core Android 9.0 Pie Car Stereo with RAM:4GB/ROM:64GB

Specifications：

General:

OS: Android 9.0 Pie

CPU: Octa-core CPU Processor

RAM: DDR3 4GB

Nand Memory: 64GB

Radio IC: NXP 6686

Bluetooth: BT 4.0

Working Voltage: 10.8~14.8V DC

Audio output: 4\*50W Max

Boot time(2nd time): about 1s

Screen:

Screen Size: 7-Inch display Screen

Resolution: 1024\*600

Capacitive Touch Screen (5 points)

Image Brightness /Contrast/ Color Adjustable

Operation System

This unit is powered by Android 9.0 system, Octa-core CPU Processor,

which will provide you a different experience than before.

EQ

**Built-in TDA7388 amplifier IC, Supports subwoofer audio output, and control it separately.**

Max audio output: 4 X 50W,

Multi-color button light

Panel buttons light RGB color are available, you can change it freely to match your car.

Phone Mirroring

Mirror your phone on the 7 inch screen.

For Android phone, you can mirror and control on the unit via USB cable connection,  
Air Play For iPhone, you can just mirror on the unit via wifi connection.

GPS：

Support online and off-line navi app, support 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/SD playback while navigating.)

DAB+ Digital Radio (Extra DAB+ box NA7001B required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle.

Which make DAB broadly accessible to most of Europe.

AV Output

For this unit, it can output almost everything to your headrests, even you play the video from USB/SD /online youtube video, Many headunits in the market can only output the DVD video to the headrest.

Bluetooth 4.0:

Built-In Microphone in the control panel for hands free calling function

External microphone also included for free clear voice calling

Support Bluetooth audio player/Phone Book function, quick search contacts.

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Support Bluetooth Connection for iPhone/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

(Attention: Only support resistance based analog signal input steering wheel)

Radio

High quality radio IC: NXP6686, with good radio reception

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in micro SD card slot/ USB Port.

Support SD card/ USB drive up to 64GB.

Support Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Support Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

OSD Language:

English, German, French, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, Thai, Hebrew, Danish，Hungarian，Dutch，Polish，Finnish，Greek，Bulgarian，Belgian，Swedish，Japanese，etc.

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034 on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI/3G internet

3G internet (Extra device required)

Support 4G internet, Require external USB 4G modem.

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

（It comes with 1.5m long WIFI antenna for better signal reception.）

Cam-In(Extra device required)

Support RCA type reverse camera input, automatically trigger to reverse camera when reversing the car.

**3.Instruction 使用说明**

**4.Package包装**

**5.Reference Link参考链接**