**深圳市帕骐电子科技有限公司**

**产品部 新品上架描述表--AA0407B**

1. **Key Features**

(Red marked content must be show on Listing Title or Bullet Point.)

**产品描述**（字体颜色为红色代表要填写在标题或者短描述。）

1. 安卓9.0系统，2+16G内存，八核cpu，更快的安装速度，更快的应用加载。高品质的6686收音IC，效果更好。

2.支持播放1080P视频，支持重低音输出，并可以单独调节，支持mirror link，可以把安卓手机、苹果手机的在线导航或者其他应用显示在机器上，支持DAB数字收音广播。

3.支持GPS功能，内置USB/SD卡槽（最大支持64GB），支持DVD全格式，内置独立Wi-Fi模块，网络连接速度更快，支持倒车摄像头功能（摄像头选配）。

4.支持快速开机，在安装好机器后，第二次开始，机器的启动时间会在1秒左右启动完成。（而其他的机器则通常需要30秒才能启动完成。）

5.购买前请先核对机子的形状和尺寸。

6.支持蓝牙通话，蓝牙音乐，支持同步电话本和支持内置外置双麦克风。

支持视频输出、OBDⅡ汽车检测功能。

Product description

1. Android 9.0 operating system, 2+16G memory, Octa-core CPU, high-quality 6686 radio IC for better AM /FM/ RDS reception.

2. Bluetooth hands-free calls, high-quality audio streaming, fast synchronization of the phone book, support for quick contact search, with built-in and external microphone, support OBDII(OBDII optional).

3.Support SD / USB or online movie sources transmit(such as Youtube).1080P HD video,subwoofer audio output and EQ setting.AV-Out function can output the DVD video to the headrest for rear passengers at the same time.support mirror link, which can display Android phone, Apple mobile phone online navigation or other applications on the car stereo.

4.Support global gps quick search function,built-in USB/SD card slot (maximum support 64GB),with built-in independent DAB module for better audio enjoyment, support reverse camera (camera optional). With built-in 16G offline map card in Germany area.

5. Support 1 second fast boot for the second time, (Other machines usually take 30 seconds to start.)

6. Please check the shape and size of the machine before purchasing.for more details,you are welcome to contact with us at any time,our support team will offer you a satisfied solution.

1. **Technical Specification技术参数**

Item Description:

7" Touchscreen Octa-Core Android 9.0 Car Stereo Player & RAM:2GB/ROM:16GB

Attention: please make sure your original car radio has the same shape as our unit.

Specifications:

General:

OS: Android 9.0

CPU:Octa-core Processor

RAM: DDR3 2GB

Nand Memory: 16GB

Radio IC: NXP TEF6686

Bluetooth: BT 4.0

Audio output: 4\*50W max

Cold Boot time: about 25-30s

Boot time(2nd time): about 1s

EQ

**Supports subwoofer audio output, and control it separately.**

Max audio output: 4 X 50W,

Signal-To-Noise Ratio: >55db

Multi-color button light

Panel buttons light RGB color are available, Already preset 7 colors of indicator buttons, you may change it freely, you can also set other colors to match your car.

Screen:

Screen Size: 7-Inch Screen

Resolution: 1024\*600

Capacitive Touch Screen (5 points)

Image Brightness /Contrast/ Color Adjustable

Phone Mirroring

Mirror your phone on the 7 inch screen.

For Android phone, you can mirror and control on the unit via USB cable connection ,
Air Play For iPhone, you can just mirror on the unit via Wi-Fi connection, cannot control

GPS:

Support online and off-line navigation app, support 3D Maps and voice guidance, your long journey will no longer be bothered by the nightmare of getting lost.

Map Storage Mode: Micro SD Card

Voice Guidance: Yes

3D Map: Yes

(Support radio/Bluetooth/USB/ playback while navigating.)

DAB+ Digital Radio (Extra DAB+ box NA7001B required)

Digital Audio Broadcasting allows you multi-regional music with your local well-known and also new channels. CD sound quality and noise-free in excellent transmission make DAB Radio a special experience in the vehicle.

which make DAB broadly accessible to most of Europe.

AV Output

Head units in the market can only output the DVD video to the headrest.

Bluetooth 4.0:

Built-In Microphone in the control panel for hands free calling function

External microphone also included for free clear voice calling

Support Bluetooth audio player/Phone Book function

(Attention: This function can only be realized when the mobile phone supports Bluetooth Audio Output/Contacts Output)

Support Bluetooth Connection for iPhones/ Most Android Phones/ Even some None Smart Phone

(Attention: The Bluetooth just for audio stream transfer, it doesn’t support file transfer or Internet tethering.)

Steering Wheel Control

Change the track, volume, etc. conveniently without taking your hands off the steering wheel, which makes your driving much safer.

(Attention: Only support resistance based analog signal input steering wheel)

Radio

AM/FM tuner built in (worldwide)

AM frequency range: 522-1620 (Europe), 530-1710 (America), 522-1620 (Russia)

FM frequency range: 87.5-108 (Europe), 87.5-107.9 (America), 65.0-108.0 (Russia)

RDS Radio: Yes

USB/SD:

Built in micro SD card slot/ USB Port

Support SD card/ USB drive up to 64GB with FAT32 or ntfs format

Support Audio Formats: MP3/WMA/WAV/APE/FLAC/OGG/AC3, etc.

Support Video Formats: RMVB/AVI/MPG/MPEG/VOB/MOV/ASF/FLV/3GP/MP4, etc.

OSD Language:

English, Russian, Spanish, Turkish, Portuguese, Arabic, Chinese, Italian, German, French, Thai,Hebrew,Danish,Hungarian,Dutch,Polish,Finnish,Greek,Bulgarian,Belgian,Swedish,

etc.

OBD2 (Extra device required)

Compatible: Most of Bluetooth type ELM327 OBD2 scanner and wifi OBD2 (Search Y0004/Y0034/VE0001B on our store)

Compatible Application: Torque

Display Data: Real-time data and trouble codes from vehicles computer.

(Attention: Few cars may not support the ECU reading accessing, those cars will not work this function.)

WIFI: Built in WIFI modem

Direct turn on WIFI function to search and connect to any free WIFI hotspots

(It comes with 1.5m long WIFI antenna for better signal reception.)

Cam-In(Extra device required)

Support RCA type reverse camera input